Cbi – clear bit immediately – Port location, bit location

Sbi- set bit immediately – Port location, bit location

Ldi temp, $f0

Out SFR, temp

Ddrb

Portb

Pin is read only register